- 6. Special Video Recording
- HLG Videos
- [Hybrid Log Gamma] settings

[Hybrid Log Gamma] settings

1Set [Rec. File Format].

[MENU/SET] [] [] [Rec. File Format] [MP4] / [MOV]

2Select a recording quality with which you can record HLG video.

[MENU/SET] [] [] [Rec Quality]

Items available for recording with HLG video are indicated as [HLG available].

Recording qualities with which you can record HLG video: List of Recording Qualities That Enable Special Videos to be Recorded

3Set [Photo Style] to [Hybrid Log Gamma].

[MENU/SET] [] [] [Photo Style] [Hybrid Log Gamma]

When the [Rec. File Format] has been set to [MOV], you can filter to show just the recording qualities where HLG video recording can be used. ([Filtering])

HLG images are shown dark on devices that do not support the HLG format. With [HDMI] / [SDI] in [HLG View Assist] of the [Custom] ([Monitor / Display]) menu, you can set the conversion method for images displayed for monitoring. ([HLG View Assist])

ISO Sensitivity When [Hybrid Log Gamma] Is Set

The lower limit of available ISO sensitivities will become [320].

The range of available ISO sensitivities is also different for [LOW] and [HIGH] in [Dual Native ISO Setting].

Reset the exposure if necessary when ISO sensitivity changes.