- 6. Special Video Recording
- Anamorphic Recording
- Anamorphic (4:3) video

Anamorphic (4:3) video

1Set [Rec. File Format] to [MOV].

[MENU/SET] [] [] [Rec. File Format] [MOV]

2Select a recording quality wherein you can record Anamorphic (4:3) video.

[MENU/SET] [] [] [Rec Quality]

Items available for recording Anamorphic (4:3) video are indicated as [ANAMOR].

Recording qualities wherein you can record Anamorphic (4:3) video: List of Recording Qualities That Enable Special Videos to be Recorded

By filtering [Rec Quality] by the number of pixels, you can display just those recording qualities that can record Anamorphic (4:3) video. ([Filtering])